# Window lifter additional requirements:

In this document, requirements requested by the stakeholder are added to the initial requirements detailed in [initial Window Lifter project requirements.](Window%20lifter%20requirements.docx)

## Window behavior:

The modules has to be able to stop the window when it is either in One Touch Up mode or in One Touch Down mode. To stop the window during an automatic mode, the following conditions must be fulfilled. **[SHR-32]**

|  |  |  |
| --- | --- | --- |
| Current mode | Button Press | Action |
| One Touch Up | Down Button | Stop One Touch Up movement **[SHR-33]** |
| One Touch Down | Up Button | Stop One Touch Down movement **[SHR-34]** |

## Antipinch functionality:

The window lifter system must include a LED to indicate the Antipinch functionality, these LED should be red and remain on during the 5s waiting. **[SHR-35]**